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SPECIFICATION FOR HANDRAILS AND SAFETY RAILING

External Handrails 

· Key clamp railing
· Galvanised uprights and fittings, yellow powder coated handrails
· No overhanging edges, rail to terminate at post with 90 degree angled fitting 
· All uprights to be evenly spaced
· The clearance between the handrail and any adjacent wall surface must be between 60mm and 75mm
· Diameter of handrail must be 42.4mm 
· For flat or ramped areas, overall height from ground level must be between 900-1000mm. For steps and stairs, overall height from the pitch line (diagonal line connecting the step nosings) must be between 900mm–1000mm.
· For steps, a handrail must be fitted to one side of a flight of steps where the flight comprises three or more risers 
· [bookmark: _GoBack]For steps wider than 1m, a handrail must be fitted on both sides.
· The loading criteria must comply with current BS regulations 
· To be fitted as per manufacturers instructions
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Edge Protection - Drops between 300mm-599mm

· Key clamp railing with crossbar
· Overall height from ground level must be 1100mm
· Spacing between ground level to crossbar and crossbar to handrail must not exceed 550mm
· Galvanised uprights and fittings with yellow powder coated handrails
· No overhanging edges, rail to terminate at post with 90 degree angled fitting 
· All uprights to be evenly spaced
· Diameter of handrail must be a minimum of 42.4mm
· The loading criteria must comply with current BS regulations 
· To be fitted as per manufacturers instructions
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Edge protection - Drops of 600mm or more

Front of properties or communal areas

· Hoop top safety fencing (style as pictured)
· Overall height from ground level must be a minimum of 1100mm
· Spacing between vertical railings must be no larger than 100mm (so a max gap of 99mm)
· Galvanised finish (or yellow powder coated for visibility requirements)
· Safety fencing to terminate with fitted post
· The loading criteria must comply with current BS regulations 
· To be fitted as per manufacturers instructions
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Rear of properties

· Flat top type safety fencing (style as pictured)
· Overall height from ground level must be a minimum of 1100mm
· Spacing between vertical railings must be no larger than 100mm (so a max gap of 99mm)
· Galvanised finish (or yellow powder coated for visibility requirements)
· Safety fencing to terminate with fitted post
· The loading criteria must comply with current BS regulations 
· To be fitted as per manufacturers instructions
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