Refurbishment works to garages at
 The Beeches, Llandysul



GARAGE REFURBISHMENT

THE WORKS.

The works will comprise of the re- roofing, installation of new garage doors, removal of ground build up around garages, the removal of all tree growth within 1.00m of all garages, and the removal and replacement of asbestos containing mastic to panel joints. Works to be carried out to the following garages – 

 1 – 29 inclusive
Total 29 garages.

PRELIMINARIES


Information

Garage Construction: Pre cast concrete panels with a profiled asbestos cement roof covering 

Making Good

The Contractor must allow in the tender sum for making good to any of the structure disturbed

Site Visits

Contractors are reminded that Officers, other than the Contract Administrator and the Clerk of Works may wish to visit the site whilst the works are on-going. Should this be the case and after suitably identifying themselves they are to be allowed unhindered access to the works.

Building Regulations

It is the responsibility of the Contractor to obtain Building Regulation approval for the works specified if required. On completion of the work a Building Regulations Completion certificate must be obtained and supplied to Barcud.

Commencement of Works

The successful Contractor will be expected to commence the works within one month of being notified of confirmation of being successful.  

Salvaged Materials

Items and materials set aside shall deem to include cleaning, inspection and selection for re-use and the removal from site of surplus materials.

The requirements of product supplier’s transferable warranties are to be adhered to. Where any of the above stipulations would be contrary to a British Standard or British Standard Code of Practice the requirements of the British Standard/Code of Practice are to prevail. Any work found not to be complying will be rectified at the Contractors expense.


GENERAL NOTES TO CONTRACTOR

When products or materials are specified in this Schedule of Works by reference to a UK standard (not implementing a European Standard of EEC or an International Standard), an equivalent guarantee will also be acceptable.

When products or materials are specified by reference to trademarks, patent, type or specific origin in these Contract Documents, the words ‘or similarly approved’ shall  be deemed to be added to such terms.

Consideration will be given to any evidence the tenderer wishes to propose in support of any claim that a product or material is equivalent to the standard or named type specified. Any foreign language documentation must be supported by a certified translation.

An equivalent product or material must be equivalent in all respects i.e. performance, appearance, colour, texture, dimensions, physical and chemical properties.

Where and to the extent that materials, products and workmanship are not fully specified they are to be:-

· Suitable for the purpose of the works stated in (or reasonable to be inferred from) the contract documents.
· In accordance with good building practise, including the relevant provisions of current BSI documents.

Contractors must satisfy themselves as to the full extent of the work to be carried out, whether mentioned in this Schedule of Works or otherwise.

Measurements and close inspections must be made to enable accurate preparation of tenders. No claims for ignorance of site conditions will be accepted. The Contractor is to include in his rates for the removal and replacement of furniture and fittings and necessary protection of the works required.

Work may be carried out beyond the normal working day provided arrangements are agreed with the Contract Administrator, particularly regarding security.



Provisional and additional work can only commence after approval in writing from the Contract Administrator.

If storage on site is required, this will be a steel lockable container for building materials and plant.

The location of this steel lockable container will be determined and agreed with the Contract Administrator. On no account, will the Contractor be allowed to use the building for the use by the labour on site.

Allow for all necessary costs associated with transporting labour and materials to an area appointed by the Contract Administrator. Storage area to be kept clean and tidy and all materials are to be removed from the site on the completion of the works.

Including for all necessary costs in conforming to the Health and Safety at Work Act 1974 and all subsequent amendments. The successful Contractor will be expected to abide by the spirit of the Act as well as its legal requirements.

All signs erected on site that are required under the current Health and Safety Regulations will be displayed at all times and they must be bi-lingual.
Contractor is to submit to the HSE an F10 form to notify HSE of the works and submit a construction phase plan to Barcud. The contractor is to Health & safety file for the duration of the works and handed over on completion of the works. All works to comply with current CDM regulations.

Allow for removing any rubbish/debris from the site as it accumulates and if required at least every other day. On completion, the whole of the works and any other adjacent areas must be left clean. 

The work must be continuous once commenced.

The Contractor must only price the items on the pricing document otherwise this may invalidate the Contractors tender.

Upon completion of the works completely clean the site including storage area, of all debris and surplus material and ensure everything is left in a safe condition.
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SCOPE OF THE WORK

Preparation


The Contractor shall liaise and meet all requirements with the appropriate utility providers to make safe and protect water mains/overhead service cables, namely electricity, telephone and television, prior to erection of scaffold.

Scaffolding to be provided to current regulations as necessary to undertake the works. Include for all works associated with bridging over obstructions such a outbuildings, porches, extensions etc. All notices and licences for scaffolding to be arranged by the Contractor. The property will not be deemed complete until scaffolding has been dismantled and removed from site.

The Contractor is to remove and re-fit all items attached to the properties, to enable the works to be carried out. Re-fitting of items to be agreed with the Contract Administrator.

All items are to be protected from damage. Where aerials and satellite dishes are installed which obstruct the working area, the Contractor is responsible for temporarily re-siting prior to the works commencing and ensuring continuity of service; subsequently re-fitting upon completion of the works.

The Contractor is to protect adjacent surfaces and buildings/properties including gardens and adjoining properties during the execution of the works.

The Contractor must ensure that all works are carried out to current regulations and supply Manufacturer’s technical fixing schedule for the roof type from “Marley” or similarly approved supplier, to the Contract Administrator.

All materials are to be stored undercover in such a manner as that they are protected from the weather at all times.

All loose items of plant are to be stored securely in a lockable enclosure at the end of each working day.

The Contractor is to allow for the use of temporary supports where deemed necessary to undertake the work safely.
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ASBESTOS REMOVAL

Carefully remove existing corrugated asbestos sheets in accordance with Asbestos Essentials guidance document a14 – Removing asbestos cement sheeting, Gutters etc.

All sheets removed to be double bagged and disposed of to asbestos licensed waste facility. Clean up all areas on completion of work and dispose of arisings as above.
All operatives to be trained in non-licensed asbestos removal with certificate supplied with tender.

Remove existing asbestos containing mastic from joints of wall panels. All work to be carried out in accordance with Asbestos Essentials guidance document a 37 – Removing asbestos containing mastic sealant.


NEW ROOF COVERING

Cover roof area with Cladco 34/1000box profile galvanized roof sheets or similar approved. Sheets to be fixed to existing concrete purlins with M8 hook bolts trimmed back to roof sheets. Bolts to be complete with sealing washers & caps.

All sheeting to be in single sheet with no laps.

Seal sheet laps with a mastic butyl tape.

Fascias, Soffits and Rainwater Good Renewal   

Remove existing rainwater goods, fascias, soffits, bargeboards. & dispose to waste facility.

Supply and fix new folded flashings at gable ends and front of buildings. Flashing to cover 2 corrugations. And be complete with drip at bottom edge.

Seal all ends of sheets with profiled foam fillers to suit 34/1000 profile.

Provide folded metal profile to cover upstand at change of level of existing garages.

Fix 150 x 18mm treated timber to lower ends of building to receive rainwater gutter.
Gutter to be 112mm wide gutters fixed with proprietary brackets at 800mm cts.
Gutters to discharge to 75mm downpipes fixed to building at 900mm cts and to discharge to existing outlets. All RWG to be in Black.

All newly rainwater goods are to be cleaned out, washed down and water tested on completion of works. Remedial works to be carried out if test fails.

Garage doors
Take out existing garage doors and dispose of to waste facility.

Supply and fix new garage doors as per Guarador Carlton up and over garage door.
Door to be complete with any necessary framing etc and complete with bottom 15mm weather seal. Door colour to be white.

Ground and tree clearance.
Excavate around garages to give min 1.00m clearance from surrounding ground.
Cut back all trees and undergrowth to give min 1.00m clearance around garages.
All arisings from the above to be removed from site to waste facility.


